Effect of Magnet Speed
A magnet is introduced into a coil (helix) of wire. The faster the magnet is moved through the coil the greater the deflection on the galvanometer.  When the magnet is introduced into the short coil slowly its deflection was a magnitude of approximately 0.15 units. When the magnet is introduced more quickly the its deflection was a magnitude of between 0.25 and 0.50 units.